{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["27 MHz"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":2,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"27 MHz","index":0,"n_rows":34,"n_cols":9,"rows_kept":34,"cut":false,"hidden":false,"merged":[[0,0,0,8]],"flags":["formulas_cached_only"]}
["27 MHz Band"]
["Kanal","Frequenz","erlaubt (D)","QD-Band","QD-Farbe",null,"Wagen","Bemerkung","Sonstiges"]
[1,26.965]
[2,26.975]
[3,26.985]
[4,26.995,"x",1,"braun "]
[5,27.005,"x"]
[6,27.015,"x"]
[7,27.025,"x"]
[8,27.035,"x"]
[9,27.045,"x",2,"rot"]
[10,27.055,"x"]
[11,27.065,"x"]
[12,27.075,"x"]
[13,27.085,"x",3,"orange"]
[14,27.095,"x"]
[15,27.105,"x"]
[16,27.115,"x"]
[17,27.125,"x"]
[18,27.135,"x"]
[19,27.145,"x",4,"gelb"]
[20,27.155]
[21,27.165]
[22,27.175]
[23,27.185]
[24,27.195,"x",5,"grün"]
[25,27.205]
[26,27.215]
[27,27.225]
[28,27.235]
[29,27.245]
[30,27.255,"x",6,"blau"]
[31,27.265]
[32,27.275]